PI40C

PI40XI

PI40XI

PI40XE

PI40XE

.

.

.

.

Figure 10.10 An implementation of the Agere switching fabric using multiple chips. The PI40XI and PI40XE consist of the same chip configured for ingress or egress.