PI40XI PI40XE PI40C .

.

.

.

.

.

.

.

Figure 10.11 Illustration of an Agere switching fabric that uses two PI40Cs and eight PI40Xs either configured for input or output. A PI40XI selects between the two PI40Cs at random.