switching fabric

1

2

N .

1

2

M .

input ports output ports

input arrives output leaves interface hardware

Figure 10.2 Illustration of a fabric that contains a separate physical data path for each interconnection. Interface hardware is needed to allow a port to specify the path for data being sent.