shared memory switching fabric controller

1

2

N .

1

2

M .

input ports output ports memory interface

Figure 10.6 Illustration of a switching fabric that uses shared memory. The memory is used to pass data; a separate hardware controller is used to pass coordination and control information.