meter 20 mbps and enqueue on AF1queue for Port 0 meter 10 mbps and enqueue on AF3queue for Port 0 meter 100mbps and enqueue on AF4queue for Port 0 meter 1 mbps and enqueue on EFqueue for Port 0 start

class EF

other class packet contains UDP/RTP/Video

packet contains UDP/RTP/Audio

other packet contents

Figure 24.7 An example decision tree for the algorithm listed in Figure 24.6 for Client 1. A vertical line represents a stage at which a decision is made, and each horizontal arrow proceeding from the vertical line represents one possible outcome.