6 6 2 46 - 1500

Dest. Address

Source Address

Frame Type Data InFrame

Header Payload

Figure 3.2 The Ethernet frame format as seen by a network system. Numbers give the size of each field measured in 8-bit octets.