Outgoing packet (to the Internet) SOURCEIP ← NATsystem IP address SOURCEPORT(or ID) ← NATNewPort (or ID) IP CHECKSUM ← Adjusted IP header checksum TCP or UDPCHECKSUM ← Adjusted transport checksum Incoming packet (from the Internet) DEST. IP Address ← Local IP Address DEST. PORT(or ID) ← Local Port (or ID) IP CHECKSUM ← Adjusted IP header checksum TCP or UDPCHECKSUM ← Adjusted transport checksum