0 8 16 24 31

ETHERNETADDRESSTYPE(1) IP ADDRESSTYPE(0800) ETHADDRLEN(6) IP ADDRLEN(4) OPERATION SENDER’SETHADDR(first 4 octets) SENDER’SETHADDR(last 2 octets) SENDER’SIP ADDR(first 2 octets) SENDER’SIP ADDR(last 2 octets) TARGET’SETHADDR(first 2 octets) TARGET’SETHADDR(last 4 octets) TARGET’SIP ADDR(all4 octets)