tag for entry state bits