08 00 45 06 00 50 00 02 ff ff ff ff ff ff 00 00

08 00 45 06 00 35 00 03 ff ff ff ff ff ff 00 00

08 00 45 06 00 50 00 00

slot #1

slot #2 key

mask

mask

Figure 14.6 An illustration of using a CAM for classification with binary values shown in hexadecimal. Only the bits covered by the mask are checked.