tag for entry state bits

Figure 19.10 A single entry in the onboard CAM divided into thirty-two tag bits used during a lookup operation, and four state bits.