0 0 0

11 10 9 8 7 6 5 4 3

state bits entry number miss

Figure 19.11 Bits the hardware returns as the result of a CAM lookup. Remaining bits are always zero.