padding (0, 128, 256, or 384 bytes)

packet data

unused space

Figure 21.2 Illustration of a packet buffer that the Intel SDK uses. The amount of padding in a given buffer is selected at random.