Outgoing packet (to the Internet) SOURCEIP ← NATsystem IP address SOURCEPORT(or ID) ← NATNewPort (or ID) IP CHECKSUM ← Adjusted IP header checksum TCP or UDPCHECKSUM ← Adjusted transport checksum

Incoming packet (from the Internet) DEST. IP Address ← Local IP Address DEST. PORT(or ID) ← Local Port (or ID) IP CHECKSUM ← Adjusted IP header checksum TCP or UDPCHECKSUM ← Adjusted transport checksum

Figure 25.10 Fields that the example NAT system changes as a packet passes from a local computer to the Internet or from the Internet to a local computer. Whenever fields in a header are changed, the corresponding checksum must be recomputed.