ISP 10.0.0.0/8 NAT router ... computers using nonroutable addresses

192.168.0.2 10.0.0.1

192.168.0.100 connection to ISP (bridged)

Figure 25.2 The connections and addresses used with an example NAT box. The local network at the site uses a net 10 prefix, and computers are assigned addresses such as 10.0.0.2, 10.0.0.3, and so on.