ME0x00 ME0x01 ME0x02

XScale

RX microblock NAT microblock TX microblock kernel thread running core component user process

running interface app.

RBUF (MSF)

TBUF (MSF) explicit buffer free for packet discard

Scratch ring for exception packets

two Scratch rings

Figure 25.5 The overall structure of the example NAT system. Except for packets discarded by the core component, all buffer allocation and deallocation operations are handled by the RX and TX microblocks.