1 2 3 4

4 3 2 1

(a)

(b) increasing memoryaddresses

increasing memoryaddresses

Figure 5.1 The arrangement of a 32-bit integer in (a) little endian and (b) big endian byte order. Bytes of the integer are numbered, with 1 representing the least significant byte and 4 representing the most significant byte.