dispatch loop packet from microengine or physical input port packet from core component on StrongARM

exception passed up to the StrongARM packet dropped packet sent to physical device or next microACE