stage 1 stage 2 stage 3 stage 4

stage 5 packets enter the pipeline packets leave the pipeline interstage packet buffer