switching fabric controller

1

2

N .

1 2 M..

input ports

output ports inactive connection active connection interface hardware

Figure 10.3 Illustration of a crossbar switching fabric shown with an active switch connecting input port 2 and output port M. The controller determines whether a switch is active or inactive.