4-input switch

(a)

SW_1 SW_3

SW_2 SW_4

"00" "01"

"10" "11"

8-input switch

(b)

4-input switch (details shown above)

4-input switch (details shown above)

SW_1

"000" "001"

SW_2

"010" "011"

SW_3

"100" "101"

SW_4

"110" "111" inputs outputs

inputs outputs

Figure 10.8 (a) Details of a 4-input Banyan switch formed by interconnecting four 2-input switching elements, and (b) an 8-input Banyan switch formed by interconnecting two 4-input switches.