input

output

MAC classify Accounting & ICMP FIB & Netflow MPLS classify AccessControl CARrouting MLPPP WRED

Figure 15.8 An illustration of how Cisco’s PXF network processor can be used. Thirty-two embedded processors are partitioned into four separate pipelines.