Contents

Address

SDRAMBus:

SDRAM Scratchpad FBICSRs Microengine xfer Microengine CSRs

AMBAxfer

Reserved

System regs

Reserved

PCIBus:

PCI memory PCI I/O PCIconfig Local PCI config

SRAMBus:

SlowPort SRAMCSRs Push/Pop cmd Locks BootROM

FFFF FFFF

C000 0000

B000 0000

A000 0000

9000 0000

8000 0000

4000 0000

0000 0000

Figure 19.2 Illustration of the thirty-two bit (i.e., 2^{32} byte) physical address space used with the StrongARM processor. The address space includes memory-mapped I/O devices as well as memories such as SRAM and SDRAM.