TFIFO

RFIFO

Pull Engine

Push Engine

CSRs

Scratch

Hash

8-entry (push)

8-entry (pull) command queues

8-entry (hash) data from SRAMtransfer registers

data to SRAMtransfer registers commands from microengine command bus commands arrive data enters

commands arrive

data leaves

Figure 20.10 A simplified illustration of the FBI architecture on Intel’s IXP1200. The Push Engine and Pull Engine operate in parallel.