dispatch loop packet from microengine or physical input port packet from core component on StrongARM

exception passed up to the StrongARM packet dropped packet sent to physical device or next microACE

Figure 25.3 Illustration of the packet sources and sinks in a typical dispatch loop used with the Intel SDK. The dispatch loop repeatedly checks each source, processes a packet, and then chooses one of the sinks for the packet.