F A B R I C fabric gasket

IXP2400 (ingress )

IXP2400 (egress ) input demux network interface

Figure 27.1 Illustration of the packet flow through two IXP2400 chips configured to handle data rates of OC-48 or higher. One chip handles ingress processing and the other handles egress.