xx x xx x xm xx x xx x xx xx x xx x xx xx x xx x xx xx x xx x xx xx x xx x xx multicast bit

Figure 3.4 The multicast bit in a 48-bit Ethernet address is the low-order bit of the high-order octet. Unicast addresses have the bit set to 0, and multicast addresses have the bit set to 1.