0 D M FLAGS bits

0 = last fragment; 1= more fragments 0 = may fragment; 1 = do not fragment Reserved (must be zero)

Figure 5.3 Bits in the FLAGS field of an IP datagram and their use in fragmentation. Most datagrams start with the three bits all set to zero.