40 80 40

fragment in reassembly buffer reassembly buffer

Figure 5.5 Illustration of the data structure used during reassembly after three fragments have arrived. Each node in the linked list contains the data length and a pointer to data in the reassembly buffer.