if (codepoint specified expedited forwarding) { Run the policing script for EF packets; Enqueue packet on the EFqueue for Port 1 } else if (packet carries UDP/RTP/video){ Run the policing script for 100 Mbps video; Enqueue packet on the AF4queue for Port 0 } else if (packet carries UDP/RTP/audio){ Run the policing script for 10 Mbps audio; Enqueue packet on the AF3queue for Port 0 } else {

Run the policing script for best-effort traffic Enqueue packet on the AF1queue for Port 0. }