multiple onboard buses queue mgmt. unit fabric proc.

table lookup

unit buffer mgmt. unit Exec. Processor pci ser. prom

. . .

CP-0 CP-1 CP-2 CP-3 CP-12 CP-13 CP-14 CP-15 clusters

SRAM fabric switching SRAM PCI bus serial PROM DRAM

connections multiplexed to physical interfaces

Figure 15.13 The internal architecture of Motorola’s C-Port chip. The diagram shows the sixteen channel processors (labeled CP-0 through CP-15) configured in parallel clusters of four channel processors per cluster.