linear array of processors (long pipeline)

to CPU channel multiplexor hash engine metering engine counter engine

TCAM engine lookaside engine 0 lookaside engine 1 lookaside engine 2 lookaside engine 3

inputs outputs external SRAM,DRAM,TCAMor coprocessors

Figure 15.16 Illustration of Xelerated’s 10q network processor architecture. The pipeline has eleven access points at which a processor can reference other functional units.